


1. Open usb upgrade software and change language to English







2、Select type as CONFIG，load file as config\_XXXXXXXXXXXXXX.ini.tar.gz




3、Click upgrade, File send completed means config file upgrade completed







4、Select type as MTD，Select files ending in .img




5、Click Upgrade，Click OK when the prompt box pops up








6、Wait for 5-8 minutes，update completed，click OK



To test this version, you need to turn off H264. You can do so from the menu.Please refer to the picture below:







Set it on off